Utiliser la commande show ip route pour vous voir les routes dans la ble de routage

R1 hostname R1 int Serial2/0 ip address 10.0.12.1 255.255.255.0 exit int Serial3/0 ip address 14.0.0.1 255.255.255.0 exit router ospf 100 network 10.0.12.0 0.0.0.255 area 0 R2 hostname R2 int Serial2/0 ip address 10.0.12.2 255.255.255.0 exit int Serial3/0 ip address 10.0.23.2 255.255.255.0 exit router ospf 100 network 10.0.12.0 0.0.0.255 area 0 network 10.0.23.0 0.0.0.255 area 0 R3 hostname R3 int Serial2/0 ip address 35.0.0.3 255.255.255.0 exit int Serial3/0 ip address 10.0.23.3 2